IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2022-06-27T09:34:37"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20210416_1515(x64) - Exporter 19.2.30.41 - Alternate UI 19.2.30.41"
Application: "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)"

People and organizations
  Person "Lana.Whittaker" of Organization (no name given)
  Owner history of Person "Lana.Whittaker" of Organization (no name given) | application "Autodesk Revit 2019 (ENG)" version "2019" identifier "Revit" by Organization "Autodesk Revit 2019 (ENG)" | change NOCHANGE | created 1656318877 (2022-06-27T08:34:37Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCELECTRICAPPLIANCETYPE "Modulo Slimline Behind The Mirror Hand Hygiene System Hand Dryer" | object type "Modulo Slimline Behind The Mirror Hand Hygiene System Hand Dryer" | names: "NBS_DudleyIndustriesLimited_HndDryrs_ModuloSlimlineBehindTheMirrorHandHygieneSystemHandDryer:Modulo Slimline Behind The Mirror Hand Hygiene System Hand Dryer:316210" | material: "NBS_DudleyIndustriesLimited_StainlessSteel_MatteBlackPowderCoated" | property sets: COBie

Types
  IFCELECTRICAPPLIANCETYPE "Modulo Slimline Behind The Mirror Hand Hygiene System Hand Dryer" | HANDDRYER | 1 occurrence | material: "NBS_DudleyIndustriesLimited_StainlessSteel_MatteBlackPowderCoated" | property sets: BOS_General, NBS_Data, IFC, COBie

Property sets
  COBie | properties | on 1 object (1 IFCFLOWTERMINAL)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_40_70_62_37:Hand dryers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Hand dryer" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Features = "Hands only" (IFCTEXT)
    Finish = "Powder-coated" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "sales@dudleyindustries.com" (IFCTEXT)
    Material = "Stainless steel" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "ModuloSlimlineBehindTheMirrorHandHygieneSystem, HandDryer" (IFCTEXT)
    Name = "HandDryers_ModuloSlimlineBehindTheMirrorHandHygieneSystem, HandDryer_DudleyIndustriesLimited" (IFCTEXT)
    NominalHeight = 328.00000049856 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 388.00000058976 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Rectangle" (IFCTEXT)
    Size = "388 x 328 x 173 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "Three year" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "Three year" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_DudleyIndustriesLimited_HandDryers_ModuloSlimlineBehindTheMirrorHandHygieneSystemHandDryer" (IFCTEXT)
    ManufacturerName = "Dudley Industries Limited" (IFCTEXT)
    ManufacturerURL = "www.dudleyindustries.com" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/nm032rjj" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_40_70_62_37" (IFCTEXT)
    Uniclass2015Title = "Hand dryers" (IFCTEXT)
    Uniclass2015Version = "Products v1.22" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Accessories = "Not required.,92405BK, Modulo Slimline Base Shelf, 600 mm.,92404BK, Modulo Slimline Base Shelf, 1200 mm" (IFCTEXT)
    BlankingPlates = "Not required.,Required" (IFCTEXT)
    BodyColour = "Matte black" (IFCTEXT)
    BodyDimensions = "388 x 328 x 173 mm" (IFCTEXT)
    BodyFinish = "Powder coated" (IFCTEXT)
    BodyIngressProtectionMinimum = "n/a" (IFCTEXT)
    BodyMaterial = "Stainless steel" (IFCTEXT)
    ContainsRedListMaterials = "n/a" (IFCTEXT)
    CountryOfMaterialOrigin = "n/a" (IFCTEXT)
    CountryOfProductManufacture = "n/a" (IFCTEXT)
    ElectricalSupplyFrequency = "50/60 Hz" (IFCTEXT)
    ElectricalSupplyPowerRating = "1.7 kW" (IFCTEXT)
    ElectricalSupplyRatedOperationalVoltageUe = "230 V a.c" (IFCTEXT)
    EmbodiedCarbon = "n/a" (IFCTEXT)
    Form = "Warm air" (IFCTEXT)
    NoiseLevelAt1MMaximum = "71 dB(A)" (IFCTEXT)
    Operation = "Automatic" (IFCTEXT)
    Recyclability = "n/a" (IFCTEXT)
    RecycledContent = "n/a" (IFCTEXT)
    Sensors = "100 mm range" (IFCTEXT)
    Standards = "n/a" (IFCTEXT)
    ThirdPartyAccreditation = "CE marked" (IFCTEXT)
    Timer = "n/a" (IFCTEXT)
    Velocity = "28 m/s" (IFCTEXT)
    Weight = "6.5 kg" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcElectricApplianceType" (IFCTEXT)
    IfcExportType = "HANDDRYER" (IFCTEXT)