IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2019-06-12T10:59:01"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20171027_0315(x64) - Exporter 17.4.0.0 - Alternate UI 17.4.0.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "KunduR" of Organization (no name given)
  Owner history of Person "KunduR" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCFLOWTERMINAL | type IFCELECTRICAPPLIANCETYPE "ModuloHandDryer" | object type "ModuloHandDryer" | names: "NBS_DudleyIndustriesLimited_HandDryers_ModuloHandDryer:ModuloHandDryer:291951" | material: "NBS_Concept" | property sets: COBie

Types
  IFCELECTRICAPPLIANCETYPE "ModuloHandDryer" | HANDDRYER | 1 occurrence | material: "NBS_Concept" | property sets: BOS_General, NBS_Data, Pset_FurnitureTypeCommon, IFC, COBie

Property sets
  COBie | properties | on 1 object (1 IFCFLOWTERMINAL)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_40_70_62_37 Hand dryers" (IFCTEXT)
    CodePerformance = "CE BS EN 60335-2-23:2003 + A1:2008 (Particular Requirements for Appliances for skin and hair Care) and BS EN60335-1:2002 + A2:2006 (incorporating A1,A11,A12, A13), (Safety of Household and similar electrical appliances), EN55014-1: 2006 + A1: 2009, EN55014-2: 1997 + A1: 2001 + A2:2008, EN61000-3-2: 2006, EN61000-3-3: 2008, RoHS, WEEE" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Automatic, energy efficient hand dryer" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "5" (IFCTEXT)
    Features = "Fits the modulo behind the mirror system, provides a hygienic, comfortable and fast hand drying solution, produces no waste, no requirement to re-stock, quiet operation at just 71 dBA, simple to install, utilises a full modular cabinet space, blanking plates available separately if required" (IFCTEXT)
    Finish = "Matte black powder coated" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Manufacturer = "tina.bowden@dudleyindustries.com" (IFCTEXT)
    Material = "Cover and back plate: CR1 CS2 steel, base plate: 1.4509 stainless steel" (IFCTEXT)
    ModelNumber = "92372BK" (IFCTEXT)
    ModelReference = "Modulo Hand Dryer" (IFCTEXT)
    Name = "HandDryers_ModuloHandDryer_DudleyIndustriesLimited" (IFCTEXT)
    NominalWidth = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "388 x 330 x 193 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "5 years" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "sales@dudleyindustries.com" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_DudleyIndustriesLimited_HandDryers_ModuloHandDryer" (IFCTEXT)
    ManufacturerName = "Dudley Industries Limited" (IFCTEXT)
    ManufacturerURL = "https://www.dudleyindustries.com/" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/0aebpxuz" (IFCTEXT)
    NBSDescription = "Hand dryers" (IFCTEXT)
    NBSReference = "45-35-72/334" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_40_70_62_37" (IFCTEXT)
    Uniclass2015Title = "Hand dryers" (IFCTEXT)
    Uniclass2015Version = "Products v1.12" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    AirVolume = "130 m³/h" (IFCTEXT)
    BodyIngressProtection = "IP21" (IFCTEXT)
    ElectricalSupplyFrequency = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    ElectricalSupplyPowerRating = "1.7kW @230 volts" (IFCTEXT)
    ElectricalSupplyRatedOperationalVoltageUe = "230 V ac" (IFCTEXT)
    Form = "High performance warm air hand dryer" (IFCTEXT)
    NoiseLevelAt1M = "71 dBA" (IFCTEXT)
    Operation = "Automatic start/stop" (IFCTEXT)
    PackingCarton = "1 piece" (IFCTEXT)
    SensorRange = "100 mm" (IFCTEXT)
    Weight = "6.5 kg" (IFCTEXT)
  Pset_FurnitureTypeCommon | properties | on 1 type object
    IsBuiltIn = TRUE (IFCBOOLEAN)
    MainColor = "n/a" (IFCTEXT)
    NominalDepth = 193.00000029336 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 330.0000005016 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 388.00000058976 (IFCLENGTHMEASURE) [MILLI METRE]
    Reference = "n/a" (IFCTEXT)
    Status = "UNSET" (IFCTEXT)
    Style = "Hand dryer" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcElectricApplianceType" (IFCTEXT)
    IfcExportType = "HANDDRYER" (IFCTEXT)