IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2019-06-12T11:52:07"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20171027_0315(x64) - Exporter 17.4.0.0 - Alternate UI 17.4.0.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "KunduR" of Organization (no name given)
  Owner history of Person "KunduR" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCFURNISHINGELEMENT | type IFCFURNITURETYPE "ModuloManualSoap" | object type "ModuloManualSoap" | names: "NBS_DudleyIndustriesLimited_SoapDpnsrs_ModuloManualSoap:ModuloManualSoap:293042" | material: "NBS_Concept" | property sets: COBie

Types
  IFCFURNITURETYPE "ModuloManualSoap" | element type "ModuloManualSoap" | 1 occurrence | material: "NBS_Concept" | property sets: BOS_General, NBS_Data, Pset_FurnitureTypeCommon, IFC, COBie

Property sets
  COBie | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    AssetIdentifier = "n/a" (IFCTEXT)
    BarCode = "n/a" (IFCTEXT)
    InstallationDate = "1900-12-31T23:59:59" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    WarrantyStartDate = "1900-12-31T23:59:59" (IFCTEXT)
  COBie | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Category = "Pr_40_70_22_81:Soap dispensers" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Black" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    Description = "Soap dispenser for effective hand cleaning, pull lever, visible below the cabinet dispensers liquid soap in, palm of hand" (IFCTEXT)
    DurationUnit = "year" (IFCTEXT)
    ExpectedLife = "10" (IFCTEXT)
    Features = "Fits the modulo behind the mirror system, reservoir is quick and easy to refill, large 1L capacity for busy washrooms, dispensing pump compatible with most liquid soap formulations, spare consumables can be conveniently stored on the shelf within the cabinet, consumables not accessible and kept free from contamination by lockable cabinet cover, lever presented to user under the cabinet with clear instructions for use, lever protrudes 80mm under cabinet, no batteries required, utilises half a modular cabinet space, blanking plates available separately if required" (IFCTEXT)
    Finish = "Matte black powder coated" (IFCTEXT)
    Grade = "Stainless Steel, EN1.4509" (IFCTEXT)
    Manufacturer = "tina.bowden@dudleyindustries.com" (IFCTEXT)
    Material = "Stainless steel" (IFCTEXT)
    ModelNumber = "92370BK" (IFCTEXT)
    ModelReference = "Modulo Manual Soap" (IFCTEXT)
    Name = "SoapDispensers_ModuloManualSoap_DudleyIndustriesLimited" (IFCTEXT)
    NominalWidth = 193.00000029336 (IFCLENGTHMEASURE) [MILLI METRE]
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "n/a" (IFCTEXT)
    Size = "193 x 280 x 193 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "10 year warranty" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  BOS_General | properties | on 1 type object
    Author = "NBS" (IFCTEXT)
    BIMObjectName = "NBS_DudleyIndustriesLimited_SoapDispensers_ModuloManualSoap" (IFCTEXT)
    ManufacturerName = "Dudley Industries Limited" (IFCTEXT)
    ManufacturerURL = "https://www.dudleyindustries.com/" (IFCTEXT)
    NBSCertification = "www.nationalbimlibrary.com/cert/lz5ep5yo" (IFCTEXT)
    NBSDescription = "Soap dispensers" (IFCTEXT)
    NBSReference = "45-35-72/358" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2015Code = "Pr_40_70_22_81" (IFCTEXT)
    Uniclass2015Title = "Soap dispensers" (IFCTEXT)
    Uniclass2015Version = "Products v1.12" (IFCTEXT)
    Version = "1" (IFCTEXT)
  NBS_Data | properties | on 1 type object
    Form = "Fits the modulo behind the mirror system" (IFCTEXT)
    MaterialsBody = "Stainless steel" (IFCTEXT)
    MaterialsFinishAndColour = "Matte black powder coated" (IFCTEXT)
    Operation = "Manual" (IFCTEXT)
  Pset_FurnitureTypeCommon | properties | on 1 type object
    IsBuiltIn = TRUE (IFCBOOLEAN)
    MainColor = "n/a" (IFCTEXT)
    NominalDepth = 193.00000029336 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 280.0000004256 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalLength = 193.00000029336 (IFCLENGTHMEASURE) [MILLI METRE]
    Reference = "n/a" (IFCTEXT)
    Status = "New" (IFCTEXT)
    Style = "Soap dispensers" (IFCTEXT)
  IFC | properties | on 1 type object
    IfcExportAs = "IfcFurnitureType" (IFCTEXT)
    IfcExportType = "NOTDEFINED" (IFCTEXT)